****************************************************************************************************
***
***		     MX2-10ADP BIOS Update Instruction
***
****************************************************************************************************

Windows update step by step:
   01) Boot to Windows.
   02) Extract BIOS update package.
   03) Open command prompt as Administrator.
   04) Change the current folder to the step 02) folder.
   05) Execute batch file run.bat.
   06) After finished, please reboot the system.

EFI update step by step:
   01) Prepare a EFI bootable USB key.
   02) Copy all files under "EfiUpdate" folder and BIOS/ME BIN file to step 01) USB key root folder.
   03) Press F7 hotkey and select step 01) EFI bootable USB key to boot.
   04) Enter the BIOS file folder and execute the batch file run.nsh.
   05) After finished, please reboot the system.

BIOS update in Setup Utility step by step:
   01) Copy BIOS ROM file in the root directory of storage device. Plug the storage device to system.
   02) Power on system and press hotkey to let system boot to Setup.
   03) Select Security page -> BIOS Update -> Path for ROM image in BIOS setup.
   04) Select the file system of storage device firstly, and select the ROM file in step 01). It will show "System is going to reboot". Press "Ok" to reboot.
   05) After system reboot, BIOS enters flash page automatically.
   06) Select "Process with flash update" to update BIOS.
   07) After finished, it would show message to ask pressing any key to reboot system.

BIOS recovery step by step:
   01) Copy BIOS ROM file in the root directory of storage device, and rename it to D892.ROM. Plug the storage device to system.
   02) Power on system and press hotkey "Ctrl+Home" to let system boot to BIOS setup recovery page.
   03) Press "Proceed with flash update" to start BIOS recovery.